#

##

##

    礦ision Build Log
    Project:
    E:\MCU目录\CA51F系列\SDK资料\SDK资料更新[2025]\CA51F2\CA51F2_SDK_【2025-12-25】\触摸功能开发包\CA51F2_Touch_DemoProj _v3.3\CA51F2_Touch_DemoProj.uvproj
    Project File Date:  12/17/2025

    Output:
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling uart.c...
    compiling interrupt.c...
    compiling debug.c...
    compiling ts_api.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=50.4 xdata=423 const=132 code=3184
    creating hex file from ".\hex\ca51fx"...
    ".\hex\ca51fx" - 0 Error(s), 0 Warning(s).