#

##

##

    礦ision Build Log
    Project:
    E:\MCU目录\CA51F系列\SDK资料\SDK资料更新[2025]\CA51F2\CA51F2_SDK_【2025-12-11】\应用实例\LCD_Simple\ca51f2.uvproj
    Project File Date:  10/23/2021

    Output:
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    *** ERROR L127: UNRESOLVED EXTERNAL SYMBOL
        SYMBOL:  LCD_Init
        MODULE:  .\output\main.obj (MAIN)
    *** ERROR L128: REFERENCE MADE TO UNRESOLVED EXTERNAL
        SYMBOL:  LCD_Init
        MODULE:  .\output\main.obj (MAIN)
        ADDRESS: 1000021H
    Program Size: data=9.0 xdata=218 const=0 code=39
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    source\lcd.c(41): warning C322: unknown identifier
    source\lcd.c(43): warning C322: unknown identifier
    source\lcd.c(54): warning C322: unknown identifier
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=130
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 3 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    source\lcd.c(41): warning C322: unknown identifier
    source\lcd.c(43): warning C322: unknown identifier
    source\lcd.c(54): warning C322: unknown identifier
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=130
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 3 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    source\lcd.c(41): warning C322: unknown identifier
    source\lcd.c(43): warning C322: unknown identifier
    source\lcd.c(54): warning C322: unknown identifier
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=130
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 3 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    compiling lcd.c...
    SOURCE\LCD.C(42): error C202: 'CKCO': undefined identifier
    SOURCE\LCD.C(42): error C141: syntax error near 'N'
    source\lcd.c - 2 Error(s), 0 Warning(s).
    compiling lcd.c...
    source\lcd.c - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=197
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=197
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=216
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=216
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    compiling lcd.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=199
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).