#

##

##

    礦ision Build Log
    Project:
    E:\MCU目录\CA51F系列\SDK资料\SDK资料更新[2025]\CA51F2\CA51F2_SDK_【2025-12-11】\应用实例\PWM_Simple\ca51f2.uvproj
    Project File Date:  10/23/2021

    Output:
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=117
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=117
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=83
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=83
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=83
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=43
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=118
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=285
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(98): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(99): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(100): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(101): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(107): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(108): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(109): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(110): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(125): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(126): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(127): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(134): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(135): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(136): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(137): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(308): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(309): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(310): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(311): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(333): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(334): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(335): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(336): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(100): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(101): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(107): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(108): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(109): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(110): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(125): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(126): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(127): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(134): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(135): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(136): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(137): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(308): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(309): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(310): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(311): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(333): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(334): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(335): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(336): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(101): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(102): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(108): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(109): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(110): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(111): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(126): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(127): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(129): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(135): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(136): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(137): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(138): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(309): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(310): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(311): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(312): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(334): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(335): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(336): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(337): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(101): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(102): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(108): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(109): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(110): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(111): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(126): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(127): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(129): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(135): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(136): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(137): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(138): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(309): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(310): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(311): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(312): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(334): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(335): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(336): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(337): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(107): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(108): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(116): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(117): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(132): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(133): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(134): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(135): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(141): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(142): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(143): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(144): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(315): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(316): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(317): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(318): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(340): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(341): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(342): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(343): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(107): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(108): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(116): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(117): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(132): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(133): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(134): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(135): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(141): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(142): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(143): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(144): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(315): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(316): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(317): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(318): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(340): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(341): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(342): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(343): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(119): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(120): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(129): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(144): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(145): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(146): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(147): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(153): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(154): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(155): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(156): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(327): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(328): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(329): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(330): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(352): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(353): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(354): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(355): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(119): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(120): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(129): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(144): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(145): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(146): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(147): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(153): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(154): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(155): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(156): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(327): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(328): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(329): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(330): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(352): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(353): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(354): error C202: 'PWMDUT_V': undefined identifier
    SOURCE\MAIN.C(355): error C202: 'PWMDUT_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(119): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(120): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(129): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(146): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(147): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(155): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(156): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(329): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(330): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(354): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(355): error C202: 'PWMDIV_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    SOURCE\MAIN.C(119): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(120): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(128): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(129): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(146): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(147): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(155): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(156): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(329): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(330): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(354): error C202: 'PWMDIV_V': undefined identifier
    SOURCE\MAIN.C(355): error C202: 'PWMDIV_V': undefined identifier
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    Target not created
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=285
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=285
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=285
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling main.c...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=282
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=184
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=220
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=261
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=258
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=258
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=258
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=261
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=261
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=261
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=261
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=259
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).
    Build target 'CA51F'
    compiling uart.c...
    compiling main.c...
    compiling delay.c...
    compiling system_clock.c...
    assembling STARTUP.A51...
    linking...
    Program Size: data=9.0 xdata=218 const=0 code=182
    creating hex file from ".\output\ca51f2"...
    ".\output\ca51f2" - 0 Error(s), 0 Warning(s).