C51 COMPILER V9.02   MAIN                                                                  12/17/2025 10:42:41 PAGE 1   


C51 COMPILER V9.02, COMPILATION OF MODULE MAIN
OBJECT MODULE PLACED IN .\output\main.obj
COMPILER INVOKED BY: D:\Keil\C51\BIN\C51.EXE source\main.c OMF2 BROWSE DEBUG PRINT(.\lst\main.lst) OBJECT(.\output\main.
                    -obj)

line level    source

   1          
   2          #ifndef _MAIN_C_
   3          #define _MAIN_C_
   4          /*********************************************************************************************************
             -************/
   5          #include "include/ca51f_config.h"               
   6          #include "include/ca51f2sfr.h"
   7          #include "include/ca51f2xsfr.h"
   8          #include "include/gpiodef_f2.h"
   9          #include "include/system_clock.h"
  10          
  11          #include "include/uart.h"
  12          #include "include/delay.h"
  13          #include "include/ext_int.h"
  14          #include <intrins.h>
  15          /*********************************************************************************************************
             -************/
  16          
  17          /***********************************************************************************
  18          函数名  ： Ext_Int_Init                                                                                 
  19          功能描述： 外部中断初始化
  20          输入参数： 无
  21          返回值  ： 无
  22          ***********************************************************************************/
  23          void Ext_Int_Init(void)                                                                 
  24          {
  25   1      #ifdef HAVE_EXINT0_EN
  26   1              Ext_Int0_Init();
  27   1      #endif  
  28   1      #ifdef HAVE_EXINT1_EN           
                      Ext_Int1_Init();
              #endif
  31   1      #ifdef HAVE_EXINT2_EN
                      Ext_Int2_Init(); 
              #endif
  34   1      #ifdef HAVE_EXINT3_EN
                      Ext_Int3_Init();
              #endif
  37   1      #ifdef HAVE_EXINT4_EN
                      Ext_Int4_Init();
              #endif
  40   1      #ifdef HAVE_EXINT5_EN
                      Ext_Int5_Init();
              #endif
  43   1      #ifdef HAVE_EXINT6_EN
                      Ext_Int6_Init();
              #endif  
  46   1      #ifdef HAVE_EXINT7_EN
                      Ext_Int7_Init();
              #endif
  49   1      #ifdef HAVE_EXINT8_EN
                      Ext_Int8_Init();
              #endif
  52   1      #ifdef HAVE_EXINT9_EN
C51 COMPILER V9.02   MAIN                                                                  12/17/2025 10:42:41 PAGE 2   

                      Ext_Int9_Init();
              #endif
  55   1      }
  56          
  57          /***********************************************************************************
  58          函数名  ： Ext_Int_Close                                                                                        
  59          功能描述： 关闭外部中断
  60          输入参数： 无
  61          返回值  ： 无
  62          ***********************************************************************************/
  63          void Ext_Int_Close(void)
  64          {
  65   1      #ifdef HAVE_EXINT0_EN
  66   1              Ext_Int0_Close();
  67   1      #endif
  68   1      #ifdef HAVE_EXINT1_EN
                      Ext_Int1_Close();
              #endif  
  71   1      #ifdef HAVE_EXINT2_EN
                      Ext_Int2_Close();
              #endif
  74   1      #ifdef HAVE_EXINT3_EN
                      Ext_Int3_Close();
              #endif
  77   1      #ifdef HAVE_EXINT4_EN
                      Ext_Int4_Close();
              #endif
  80   1      #ifdef HAVE_EXINT5_EN
                      Ext_Int5_Close();
              #endif  
  83   1      #ifdef HAVE_EXINT6_EN
                      Ext_Int6_Close();
              #endif  
  86   1      #ifdef HAVE_EXINT7_EN
                      Ext_Int7_Close();
              #endif
  89   1      #ifdef HAVE_EXINT8_EN
                      Ext_Int8_Close();
              #endif
  92   1      #ifdef HAVE_EXINT9_EN
                      Ext_Int9_Close();
              #endif
  95   1      }
  96          
  97          /*********************************************************************************************************
             -************/
  98          
  99          void main(void)
 100          {
 101   1      #ifdef LVD_RST_ENABLE
 102   1              LVDCON = 0xE1;                                  //设置LVD复位电压为2V
 103   1      #endif
 104   1      
 105   1      #if (SYSCLK_SRC == PLL)
                      Sys_Clk_Set_PLL(PLL_Multiple);  //设置系统时钟为PLL，PLL_Multiple为倍频倍数
              #endif
 108   1              
 109   1      #ifdef UART0_EN
                      Uart0_Initial(UART0_BAUTRATE);  //初始化UART0
              #endif
 112   1              
 113   1      #ifdef UART1_EN
C51 COMPILER V9.02   MAIN                                                                  12/17/2025 10:42:41 PAGE 3   

                      Uart1_Initial(UART1_BAUTRATE);  //初始化UART1
              #endif
 116   1      
 117   1      #ifdef UART2_EN
                      Uart2_Initial(UART2_BAUTRATE);  //初始化UART2
              #endif
 120   1              
 121   1              EA = 1;                                                 //开全局中断
 122   1              Ext_Int_Init();
 123   1      
 124   1      #ifdef PRINT_EN
                      uart_printf("INT0 to INT9 Demo Code\n");
              #endif
 127   1              
 128   1              while(1)
 129   1              {
 130   2                      
 131   2              }
 132   1      }
 133          #endif
 134          


MODULE INFORMATION:   STATIC OVERLAYABLE
   CODE SIZE        =     16    ----
   CONSTANT SIZE    =   ----    ----
   XDATA SIZE       =   ----    ----
   PDATA SIZE       =   ----    ----
   DATA SIZE        =   ----    ----
   IDATA SIZE       =   ----    ----
   BIT SIZE         =   ----    ----
   EDATA SIZE       =   ----    ----
   HDATA SIZE       =   ----    ----
   XDATA CONST SIZE =   ----    ----
   FAR CONST SIZE   =   ----    ----
END OF MODULE INFORMATION.


C51 COMPILATION COMPLETE.  0 WARNING(S),  0 ERROR(S)
